       Release Notes for Version 17.03.00 of the J1699-3 software


Except for the issues detailed in 'J1633-3 Work Status', this release includes the
requirements of revision 17.3 of the J1699-3 document and is intended to
test Model Year 2020 and beyond.



NOTES:
 - Slow PCs/J2534 devices may cause false vehicle failures!
 - For EOBD ONLY, scanning CAN baud rates may cause ECUs to go BUS_OFF!
 - This release only supports the 0404 version of the J2534 API!
 - The file "J1699 User Notes.doc" is a simple User Guide to the J1699-3 software.
 - To avoid false failures during the CARB Drive Cycle, do NOT operate the vehicle at exactly 25 MPH (40KPH).


Version 17.03.00 adds the following features:
Issue #     Description
1033        Change wording for Prompt Q03 to clarify VIN model year.
1034        Improve wording of 2022-2024 phase-in warning and failure

Version 17.03.00 fixes the following issues:
Issue #     Description
1025        Fix sections of information missing from logfile.
1026        Fix false failure of SID $8 support request.
1027        INF $78 is required by only US medium duty and heavy duty diesel vehicles.
1028        Remove extra space between "****" and other text.
1029        Fix display of IUMPR data.
1030        Fix problems with use of pFEOCNTR causing application to crash.
1031        Fix waiting for unsupported bank completion.
1032        China6 allows ECUs to reply both positively and negatively to Clear Codes request when engine running.

