       Release Notes for Version 17.04.02 of the J1699-3 software


Except for the issues detailed in 'J1633-3 Work Status', this release includes the
requirements of revision 17.4 of the J1699-3 document and is intended to
test Model Year 2022 and beyond.



NOTES:
 - Slow PCs/J2534 devices may cause false vehicle failures!
 - For EOBD ONLY, scanning CAN baud rates may cause ECUs to go BUS_OFF!
 - This release only supports the 0404 version of the J2534 API!
 - The file "J1699 User Notes.doc" is a simple User Guide to the J1699-3 software.
 - To avoid false failures during the CARB Drive Cycle, do NOT operate the vehicle at exactly 25 MPH (40KPH).


Version 17.04.02 adds the following features:
Issue #     Description

Version 17.04.02 fixes the following issues:
Issue #     Description
1044        Fix false failures for SID $1 PID $01 and $41 GPF support for US and EU vehicles.
1062        Fix false failures for required support of SID $9 INF $78.
1063        Fix false failures for required support of SID $9 INF $77.
