       Release Notes for Version 16.02.03 of the J1699-3 software


Except for the issues detailed in SourceForge, this release includes the
requirements of revision 16.2 of the J1699-3 document and is intended to
test Model Year 2018 and beyond.



NOTES:
 - Slow PCs/J2534 devices may cause false vehicle failures!
 - For EOBD ONLY, scanning CAN baud rates may cause ECUs to go BUS_OFF!
 - This release only supports the 0404 version of the J2534 API!
 - The file "J1699 User Notes.doc" is a simple User Guide to the J1699-3 software.
 - To avoid false failures during the CARB Drive Cycle, do NOT operate the vehicle at exactly 25 MPH (40KM/H).


Version 16.02.03 adds the following features:
270         Evaluation of PKE and EOE commented out until evaluation criteria confirmed.



Version 16.02.03 corrects the following bugs:
Issue #     Description
384         Initialize ECU_Data_index to prevent program failure.
385         Fix the scaling of DT, FC, EOE, CDEODT, CDERDT, CIDT, CDFC, CIFC, CDEOGE, CDERGE, GE





NOTES ON CHANGES:

Issue 259 - INFs $21-$29 data is displayed but not evaluated, pending confirmation
            of the evaluation criteria in the j1699-3 document.
