       Release Notes for Version 16.07.04 of the J1699-3 software


Except for the issues detailed in SourceForge, this release includes the
requirements of revision 16.7 Ballot REV2 of the J1699-3 document and is intended to
test Model Year 2021 and beyond.



NOTES:
 - Slow PCs/J2534 devices may cause false vehicle failures!
 - For EOBD ONLY, scanning CAN baud rates may cause ECUs to go BUS_OFF!
 - This release only supports the 0404 version of the J2534 API!
 - The file "J1699 User Notes.doc" is a simple User Guide to the J1699-3 software.
 - To avoid false failures during the CARB Drive Cycle, do NOT operate the vehicle at exactly 25 MPH (40KM/H).


Version 16.07.04 adds no new features


Version 16.07.04 fixes the following issues:
Issue #     Description
424         Fix erroneous failures of ECUs which do not support SID $4.
425         Fix SID $9 INF $8 data size and NODI check to prevent false pass.
426         Add prompts for key on and key off in the Vehicle Report test.
